{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["遥测","遥信","遥脉","遥控","遥调"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"遥测","index":0,"n_rows":13,"n_cols":67,"rows_kept":13,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","描述","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]
["device_1","YC0","type","读数据","读写","1.0","0.0","--","0","0","字符串","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC1","year","读数据","读写","1.0","0.0","--","0","1","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC2","mon","读数据","读写","1.0","0.0","--","0","2","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC3","day","读数据","读写","1.0","0.0","--","0","3","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC4","hour","读数据","读写","1.0","0.0","--","0","4","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC5","min","读数据","读写","1.0","0.0","--","0","5","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC6","sec","读数据","读写","1.0","0.0","--","0","6","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC7","钟差值(秒)","读数据","读写","1.0","0.0","--","0","7","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC8","工频钟hour","读数据","读写","1.0","0.0","--","0","8","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC9","工频钟min","读数据","读写","1.0","0.0","--","0","9","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC10","工频钟sec","读数据","读写","1.0","0.0","--","0","10","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]
["device_1","YC11","工频","读数据","读写","1.0","0.0","--","0","11","16位有符号","12","0.0","否","否","0","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","","","","关","1000","0","原始值*系数+偏移","禁用","","","","","","","","","","","","","","",""]

{"sheet":"遥信","index":1,"n_rows":1,"n_cols":67,"rows_kept":1,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","描述","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]

{"sheet":"遥脉","index":2,"n_rows":1,"n_cols":67,"rows_kept":1,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","描述","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]

{"sheet":"遥控","index":3,"n_rows":1,"n_cols":67,"rows_kept":1,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","描述","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]

{"sheet":"遥调","index":4,"n_rows":1,"n_cols":67,"rows_kept":1,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","描述","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]