{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["模拟量","开关量"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"模拟量","index":0,"n_rows":18,"n_cols":67,"rows_kept":18,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","物模型标识(测点描述)","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]
["设备1","YC0","机内空气温度(℃)","读实时数据","读写","0.1","0.0","--","0","0","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","机内空气温度","10","关","","","","禁用","","","","","","","","","","","","","","","","204"]
["设备1","YC1","直流电压1(V)","读实时数据","读写","0.1","0.0","--","0","1","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","直流电压1","10","关","","","","禁用","","","","","","","","","","","","","","","","207"]
["设备1","YC2","直流电压2(V)","读实时数据","读写","0.1","0.0","--","0","2","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","直流电压2","10","关","","","","禁用","","","","","","","","","","","","","","","","225"]
["设备1","YC3","直流电流1(A)","读实时数据","读写","0.1","0.0","--","0","3","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","直流电流1","10","关","","","","禁用","","","","","","","","","","","","","","","","208"]
["设备1","YC4","直流电流2(A)","读实时数据","读写","0.1","0.0","--","0","4","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","直流电流2","10","关","","","","禁用","","","","","","","","","","","","","","","","230"]
["设备1","YC5","总发电量(kWh)","读实时数据","读写","0.1","0.0","--","0","5","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","总发电量","10","关","","","","禁用","","","","","","","","","","","","","","","","202"]
["设备1","YC6","总运行时间(h)","读实时数据","读写","1.0","0.0","--","0","7","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","总运行时间","1","关","","","","禁用","","","","","","","","","","","","","","","","203"]
["设备1","YC7","总有功功率(W)","读实时数据","读写","1.0","0.0","--","0","9","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","总有功功率","1","关","","","","禁用","","","","","","","","","","","","","","","","219"]
["设备1","YC8","日发电量(kWh)","读实时数据","读写","0.01","0.0","--","0","10","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","日发电量","10","关","","","","禁用","","","","","","","","","","","","","","","","201"]
["设备1","YC9","A相电流(A)","读实时数据","读写","0.1","0.0","--","0","11","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","A相电流","10","关","","","","禁用","","","","","","","","","","","","","","","","213"]
["设备1","YC10","A相电压(V)","读实时数据","读写","0.1","0.0","--","0","12","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","A相电压","10","关","","","","禁用","","","","","","","","","","","","","","","","210"]
["设备1","YC11","电网频率(Hz)","读实时数据","读写","0.01","0.0","--","0","13","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","电网频率","10","关","","","","禁用","","","","","","","","","","","","","","","","222"]
["设备1","YC12","B相电流(A)","读实时数据","读写","0.1","0.0","--","0","14","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","B相电流","10","关","","","","禁用","","","","","","","","","","","","","","","","214"]
["设备1","YC13","B相电压(V)","读实时数据","读写","0.1","0.0","--","0","15","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","B相电压","10","关","","","","禁用","","","","","","","","","","","","","","","","211"]
["设备1","YC14","C相电流(A)","读实时数据","读写","0.1","0.0","--","0","16","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","C相电流","10","关","","","","禁用","","","","","","","","","","","","","","","","215"]
["设备1","YC15","C相电压(V)","读实时数据","读写","0.1","0.0","--","0","17","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","C相电压","10","关","","","","禁用","","","","","","","","","","","","","","","","212"]
["设备1","YC16","状态(--)","读实时数据","读写","1.0","0.0","--","0","18","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","90.0","20.0","10.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","状态","1","关","","","","禁用","","","","","","","","","","","","","","","","224"]

{"sheet":"开关量","index":1,"n_rows":1,"n_cols":67,"rows_kept":1,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","物模型标识(测点描述)","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]