{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["模拟量","开关量"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"模拟量","index":0,"n_rows":43,"n_cols":67,"rows_kept":43,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","物模型标识(测点描述)","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]
["YG1","DE","日发电量","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5002","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","日发电量","10","关","","","","禁用","","","","","","","","","","","","","","","","201"]
["YG1","TE","总发电量","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","5003","32位无符号","3412","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","总发电量","10","关","","","","禁用","","","","","","","","","","","","","","","","202"]
["YG1","RUNT","运行时间","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","5005","32位无符号","3412","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","总运行时间","1","关","","","","禁用","","","","","","","","","","","","","","","","203"]
["YG1","Temp","机内温度","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5007","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","机内空气温度","10","关","","","","禁用","","","","","","","","","","","","","","","","204"]
["YG1","Upv1","直流电压1","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5010","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","直流电压1","10","关","","","","禁用","","","","","","","","","","","","","","","","207"]
["YG1","Ipv1","直流电流1","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5011","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","直流电流1","10","关","","","","禁用","","","","","","","","","","","","","","","","208"]
["YG1","Upv2","直流电压2","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5012","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","直流电压2","10","关","","","","禁用","","","","","","","","","","","","","","","","225"]
["YG1","Ipv2","直流电流2","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5013","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","直流电流2","10","关","","","","禁用","","","","","","","","","","","","","","","","230"]
["YG1","Pdc","总直流功率","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","5016","32位无符号","3412","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","总直流功率","1","关","","","","禁用","","","","","","","","","","","","","","","","209"]
["YG1","Upv3","直流电压3","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5014","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","直流电压3","10","关","","","","禁用","","","","","","","","","","","","","","","","226"]
["YG1","Ipv3","直流电流3","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5015","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","直流电流3","10","关","","","","禁用","","","","","","","","","","","","","","","","231"]
["YG1","Ua","A相电压","0x04号命令(读输入寄存器)","读写","0.05773","0.0","--","0","5018","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","A相电压","10","关","","","","禁用","","","","","","","","","","","","","","","","210"]
["YG1","Ub","B相电压","0x04号命令(读输入寄存器)","读写","0.05773","0.0","--","0","5019","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","B相电压","10","关","","","","禁用","","","","","","","","","","","","","","","","211"]
["YG1","Uc","C相电压","0x04号命令(读输入寄存器)","读写","0.05773","0.0","--","0","5020","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","C相电压","10","关","","","","禁用","","","","","","","","","","","","","","","","212"]
["YG1","Ia","A相电流","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5021","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","A相电流","10","关","","","","禁用","","","","","","","","","","","","","","","","213"]
["YG1","Ib","B相电流","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5022","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","B相电流","10","关","","","","禁用","","","","","","","","","","","","","","","","214"]
["YG1","Ic","C相电流","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5023","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","C相电流","10","关","","","","禁用","","","","","","","","","","","","","","","","215"]
["YG1","P","总有功功率","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","5030","32位无符号","3412","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","总有功功率","1","关","","","","禁用","","","","","","","","","","","","","","","","219"]
["YG1","Q","总无功功率","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","5032","32位无符号","3412","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","总无功功率","1","关","","","","禁用","","","","","","","","","","","","","","","","220"]
["YG1","COS","功率因数","0x04号命令(读输入寄存器)","读写","0.001","0.0","--","0","5034","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","总功率因数","1","关","","","","禁用","","","","","","","","","","","","","","","","221"]
["YG1","F","频率","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","5035","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","电网频率","10","关","","","","禁用","","","","","","","","","","","","","","","","222"]
["YG1","Status","状态","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","5037","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","状态","1","关","","","","禁用","","","","","","","","","","","","","","","","224"]
["YG1","Upv4","直流电压4","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","1","5114","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","直流电压4","10","关","","","","禁用","","","","","","","","","","","","","","","","227"]
["YG1","Ipv4","直流电流4","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","1","5115","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0","直流电流4","10","关","","","","禁用","","","","","","","","","","","","","","","","232"]
["YG1","Upv5","直流电压5","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","1","5116","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","否","0","直流电压5","10","关","","","","禁用","","","","","","","","","","","","","","","","228"]
["YG1","Ipv5","直流电流5","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","1","5117","16位有符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","否","0","直流电流5","10","关","","","","禁用","","","","","","","","","","","","","","","","233"]
["YG1","I1","第一路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7012","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流1","10","关","","","","禁用","","","","","","","","","","","","","","","","274"]
["YG1","I2","第二路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7013","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流2","10","关","","","","禁用","","","","","","","","","","","","","","","","275"]
["YG1","I3","第三路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7014","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流3","10","关","","","","禁用","","","","","","","","","","","","","","","","276"]
["YG1","I4","第四路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7015","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流4","10","关","","","","禁用","","","","","","","","","","","","","","","","277"]
["YG1","I5","第五路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7016","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流5","10","关","","","","禁用","","","","","","","","","","","","","","","","278"]
["YG1","I6","第六路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7017","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流6","10","关","","","","禁用","","","","","","","","","","","","","","","","279"]
["YG1","I7","第七路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7018","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流7","10","关","","","","禁用","","","","","","","","","","","","","","","","280"]
["YG1","I8","第八路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7019","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流8","10","关","","","","禁用","","","","","","","","","","","","","","","","281"]
["YG1","I9","第九路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7020","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流9","10","关","","","","禁用","","","","","","","","","","","","","","","","282"]
["YG1","I10","第十路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7021","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流10","10","关","","","","禁用","","","","","","","","","","","","","","","","283"]
["YG1","I11","第十一路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7022","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流11","10","关","","","","禁用","","","","","","","","","","","","","","","","284"]
["YG1","I12","第十二路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7023","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流12","10","关","","","","禁用","","","","","","","","","","","","","","","","285"]
["YG1","I13","第十三路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7024","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流13","10","关","","","","禁用","","","","","","","","","","","","","","","","286"]
["YG1","I14","第十四路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7025","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流14","10","关","","","","禁用","","","","","","","","","","","","","","","","287"]
["YG1","I15","第十五路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7026","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","汇流板电流15","10","关","","","","禁用","","","","","","","","","","","","","","","","288"]
["YG1","I16","第十六路电流","0x04号命令(读输入寄存器)","只读","0.01","0.0","--","3","7027","16位无符号","12","0.0","否","否","512","0","采集点","否","0","0","否","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","60","0.5","是","0","无","10","关","","","","禁用","","","","","","","","","","","","","","","","289"]

{"sheet":"开关量","index":1,"n_rows":95,"n_cols":67,"rows_kept":95,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","物模型标识(测点描述)","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]
["YG1","YX1","电网过压","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","2","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX2","电网过压","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","3","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX3","电网欠压","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","4","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX4","电网欠压","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","5","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX5","硬件故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","6","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX6","电网过频","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","8","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX7","电网欠频","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","9","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX8","孤岛","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","10","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX9","直流分量超标","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","11","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX10","漏电流超标","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","12","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX11","电网异常","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","13","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX12","电网过压","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","14","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX13","电网过压","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","15","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX14","PV 组件过载","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","16","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX15","电网电压不平衡","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","17","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX16","母线电压高","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","19","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX17","母线电压高","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","20","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX18","过流保护","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","21","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX19","过流保护","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","22","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX20","光伏输入配置在逆变器运行时改变","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","23","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX21","母线电压不平衡","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","24","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX22","母线电压不平衡","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","25","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX23","母线电压不平衡","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","26","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX24","模块温度过高","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","36","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX25","环境温度过高","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","37","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX26","继电器故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","38","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX27","系统绝缘阻抗低","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","39","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX28","过流保护","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","40","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX29","硬件故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","41","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX30","硬件故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","42","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX31","环境温度低","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","43","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX32","交直流逆变电路故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","44","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX33","光伏输入配置模式设置与实际连接不符","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","47","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX34","硬件故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","48","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX35","硬件故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","49","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX36","硬件故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","50","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX37","硬件过压过流保护","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","51","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX38","风扇故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","70","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX39","交流侧SPD告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","71","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX40","直流侧SPD告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","72","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX41","通讯故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","74","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX42","光照不足","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","75","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX43","PV过载","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","76","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX44","PV1异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","78","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX45","PV2异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","79","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX46","PV3异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","80","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX47","PV4异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","81","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX48","AFD模块异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","87","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX49","电弧故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","88","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX50","AFD关闭告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","89","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX51","组串1反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","532","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX52","组串2反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","533","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX53","组串3反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","534","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX54","组串4反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","535","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX55","组串5反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","536","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX56","组串6反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","537","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX57","组串7反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","538","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX58","组串8反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","539","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX59","组串9反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","540","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX60","组串10反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","541","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX61","组串11反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","542","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX62","组串12反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","543","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX63","组串13反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","544","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX64","组串14反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","545","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX65","组串15反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","546","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX66","组串16反接告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","547","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX67","组串1组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","548","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX68","组串2组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","549","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX69","组串3组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","550","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX70","组串4组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","551","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX71","组串5组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","552","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX72","组串6组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","553","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX73","组串7组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","554","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX74","组串8组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","555","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX75","组串9组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","556","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX76","组串10组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","557","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX77","组串11组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","558","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX78","组串12组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","559","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX79","组串13组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","560","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX80","组串14组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","561","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX81","组串15组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","562","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX82","组串16组件异常告警","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","2","5044","16位无符号","12","0.0","否","是","563","1","采集点","否","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX83","运行","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","0","0","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","否","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX84","停机","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","1","1","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX85","按键关机","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","3","3","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX86","紧急停机","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","5","5","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX87","待机","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","4","4","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","否","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX88","初始待机","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","2","2","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","否","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX89","启动中","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","6","6","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","否","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX90","告警运行","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","10","10","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX91","降额运行","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","11","11","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX92","调度运行","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","12","12","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX93","故障运行","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","9","9","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]
["YG1","YX94","通信故障","0x04号命令(读输入寄存器)","只读","1.0","0.0","--","4","5080","16位无符号","12","0.0","否","否","512","0","采集点","是","13","13","是","否","否","否","否","100.0","90.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","模拟量报警","开关变位","通知","否","周期存储","60","0.5","是","0",null,"1","关","","","","禁用","","","","","","","","","","","","","","","","-1"]