{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["模拟量","开关量"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"模拟量","index":0,"n_rows":23,"n_cols":67,"rows_kept":23,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","物模型标识(测点描述)","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]
["INV1","P","ep","0x04号命令(读输入寄存器)","读写","0.01","0.0","--","0","1050","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","有功功率","0","关","","","","禁用","","","","","","","","","","","","","","","","17"]
["INV1","Q","eq","0x04号命令(读输入寄存器)","读写","0.01","0.0","--","0","1051","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","无功功率","0","关","","","","禁用","","","","","","","","","","","","","","","","18"]
["INV1","PF","cos","0x04号命令(读输入寄存器)","读写","0.001","0.0","--","0","1052","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","功率因数","0","关","","","","禁用","","","","","","","","","","","","","","","","28"]
["INV1","Ua","ua","0x04号命令(读输入寄存器)","读写","0.057737","0.0","--","0","1053","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","A相电压","0","关","","","","禁用","","","","","","","","","","","","","","","","9"]
["INV1","Ub","ub","0x04号命令(读输入寄存器)","读写","0.057737","0.0","--","0","1054","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","B相电压","0","关","","","","禁用","","","","","","","","","","","","","","","","10"]
["INV1","Uc","uc","0x04号命令(读输入寄存器)","读写","0.057737","0.0","--","0","1055","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","C相电压","0","关","","","","禁用","","","","","","","","","","","","","","","","11"]
["INV1","F","f","0x04号命令(读输入寄存器)","读写","0.01","0.0","--","0","1056","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","频率","0","关","","","","禁用","","","","","","","","","","","","","","","","32"]
["INV1","Ia","ia","0x04号命令(读输入寄存器)","读写","0.01","0.0","--","0","1057","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","A相电流","0","关","","","","禁用","","","","","","","","","","","","","","","","0"]
["INV1","Ib","ib","0x04号命令(读输入寄存器)","读写","0.01","0.0","--","0","1058","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","B相电流","0","关","","","","禁用","","","","","","","","","","","","","","","","1"]
["INV1","Ic","ic","0x04号命令(读输入寄存器)","读写","0.01","0.0","--","0","1059","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","C相电流","0","关","","","","禁用","","","","","","","","","","","","","","","","2"]
["INV1","Pdc","inputep","0x04号命令(读输入寄存器)","读写","0.01","0.0","--","0","1068","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","直流功率","0","关","","","","禁用","","","","","","","","","","","","","","","","164"]
["INV1","Umppt1","uPV1","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","1073","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","MPPT电压1","1","关","","","","禁用","","","","","","","","","","","","","","","","1350"]
["INV1","Umppt2","uPV2","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","1074","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","MPPT电压2","2","关","","","","禁用","","","","","","","","","","","","","","","","2351"]
["INV1","Umppt3","uPV3","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","1075","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","MPPT电压3","3","关","","","","禁用","","","","","","","","","","","","","","","","3352"]
["INV1","Umppt4","uPV4","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","1076","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","MPPT电压4","4","关","","","","禁用","","","","","","","","","","","","","","","","4353"]
["INV1","Imppt1","iPV1","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","1081","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","不报警","通知","否","周期存储","300","1.0","是","0","MPPT电流1","1","关","","","","禁用","","","","","","","","","","","","","","","","1344"]
["INV1","Imppt2","iPV2","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","1082","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","MPPT电流2","2","关","","","","禁用","","","","","","","","","","","","","","","","2345"]
["INV1","Imppt3","iPV3","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","1083","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","MPPT电流3","3","关","","","","禁用","","","","","","","","","","","","","","","","3346"]
["INV1","Imppt4","iPV4","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","1084","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","MPPT电流4","4","关","","","","禁用","","","","","","","","","","","","","","","","4347"]
["INV1","Temp","temperature","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","1082","16位有符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","温度","0","关","","","","禁用","","","","","","","","","","","","","","","","36"]
["INV1","DayE","daypositiveActice","0x04号命令(读输入寄存器)","读写","0.1","0.0","--","0","1100","16位无符号","12","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","日发电量","0","关","","","","禁用","","","","","","","","","","","","","","","","238"]
["INV1","TotalE","positiveActice","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","1101","32位无符号","1234","0.0","否","否","512","1","采集点","否","0","0","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0","温度过高","0","关","","","","禁用","","","","","","","","","","","","","","","","240"]

{"sheet":"开关量","index":1,"n_rows":9,"n_cols":67,"rows_kept":9,"flags":["formulas_cached_only"]}
["设备名称(DevName)","测点名称(TagName)","物模型标识(测点描述)","功能码","读写属性","系数K","偏移B","变量单位","测点分组","寄存器地址","数据类型","高低位顺序","初始值","是否取反","数值转换","原始值","转换值","测点来源","按位取值","取值起始位","取值终止位","报警使能","是否开启高高报警","是否开启高报警","是否开启低报警","是否开启低低报警","高高报警限值","高报警限值","低报警限值","低低报警限值","高高报警消息","高报警消息","低报警消息","低低报警消息","报警死区","开关报警类型","开关报警消息","报警等级","存储使能","存储类型","存储间隔(s)","压缩存储精度","是否上传","辅助参数","PV上传标识","PV上传系数","限值使能位","最大值","最小值","公式计算","控制模式","遥调功能码","遥调寄存器地址","遥调数据类型","遥调字节序","定值组功能码","控分功能码","控分寄存器","控分选择值","控分执行值","控分撤销值","控合功能码","控合寄存器","控合选择值","控合执行值","控合撤销值","Pv码(优先)"]
["上能逆变器4","上能逆变器4_电网电压异常","warning1","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","2030","16位无符号","12","0.0","否","否","512","1","采集点","是","14","14","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0",null,"0","关","","","","禁用","","","","","","","","","","","","","","","","100010"]
["上能逆变器4","上能逆变器4_电网频率异常","warning2","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","2030","16位无符号","12","0.0","否","否","512","1","采集点","是","15","15","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0",null,"0","关","","","","禁用","","","","","","","","","","","","","","","","100013"]
["上能逆变器4","上能逆变器4_电网异常","warning3","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","2030","16位无符号","12","0.0","否","否","512","1","采集点","是","6","6","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0",null,"0","关","","","","禁用","","","","","","","","","","","","","","","","100006"]
["上能逆变器4","上能逆变器4_残余电流超限","warning4","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","2030","16位无符号","12","0.0","否","否","512","1","采集点","是","8","8","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0",null,"0","关","","","","禁用","","","","","","","","","","","","","","","","100016"]
["上能逆变器4","上能逆变器4_绝缘阻抗异常","warning5","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","2030","16位无符号","12","0.0","否","否","512","1","采集点","是","7","7","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0",null,"0","关","","","","禁用","","","","","","","","","","","","","","","","100018"]
["上能逆变器4","上能逆变器4_隆额运行","warning6","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","2030","16位无符号","12","0.0","否","否","512","1","采集点","是","2","2","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0",null,"0","关","","","","禁用","","","","","","","","","","","","","","","","100266"]
["上能逆变器4","上能逆变器4_故障","warning7","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","2030","16位无符号","12","0.0","否","否","512","1","采集点","是","4","4","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0",null,"0","关","","","","禁用","","","","","","","","","","","","","","","","100265"]
["上能逆变器4","上能逆变器4_过温运行","warning8","0x04号命令(读输入寄存器)","读写","1.0","0.0","--","0","2030","16位无符号","12","0.0","否","否","512","1","采集点","是","11","11","否","否","否","否","否","100.0","100.0","10.0","0.0","高高报警","高报警","低报警","低低报警","0.0","变位报警","开关变位","通知","否","周期存储","300","1.0","是","0",null,"0","关","","","","禁用","","","","","","","","","","","","","","","","100019"]